?UNDEF TIME-DIV
  [IF]  100e-6     FVALUE TIME-DIV
   	50e        FVALUE I-GAIN
 	0.009703e  FVALUE I-OFFSET
	: SPOINTS ( n -- ) DROP #5000 POINTS ;
[THEN]

S" UHP VI"             SET-1STTITLE
S" GTA measurements"   SET-2NDTITLE

graph-id# 1 = [IF] -0.0199811e -250e  0.179979e 250e DIMENSIONS 
		   0 TO X-col  S" Time [s]"  SET-HLABEL
		   2 TO Y-col  S" Vla"       SET-VLABEL
		   S" 1kHz source frequency" SET-IXLINE
	    [THEN]

graph-id# 2 = [IF] -0.0199811e -0.05e 0.179979e 0.05e DIMENSIONS
		   0 TO X-col  S" Time [s]"  SET-HLABEL
		   1 TO Y-col  S" Ila"       SET-VLABEL
		   S" 1kHz source frequency" SET-IXLINE
	    [THEN]


graph-id# 3 = [IF] -0.0499783e -550e 0.449922e 550e DIMENSIONS
		   0 TO X-col  S" Time [s]"   SET-HLABEL
		   2 TO Y-col  S" Vla"        SET-VLABEL
		   S" 50 Hz source frequency" SET-IXLINE
	    [THEN]

graph-id# 4 = [IF] -0.0499783e -0.05e 0.449922e 0.05e DIMENSIONS
		   0 TO X-col  S" Time [s]"   SET-HLABEL
		   1 TO Y-col  S" Ila"        SET-VLABEL
		   S" 50 Hz source frequency" SET-IXLINE
	    [THEN]

graph-id# 5 = [IF] -0.0499892e -550e  0.4499110e 550e DIMENSIONS
		   0 TO X-col  S" Time [s]"   SET-HLABEL
		   2 TO Y-col  S" Vla"        SET-VLABEL
		   S" 50 Hz source frequency" SET-IXLINE
	    [THEN]

graph-id# 6 = [IF] -0.0499892e -0.05e  0.4499110e 0.05e DIMENSIONS
		   0 TO X-col  S" Time [s]"   SET-HLABEL
		   1 TO Y-col  S" Ila"        SET-VLABEL
		   S" 50 Hz source frequency" SET-IXLINE
	    [THEN]

graph-id# 7 = [IF] -0.49913e -550e  4.49987e 550e DIMENSIONS
		   0 TO X-col  S" Time [s]"   SET-HLABEL
		   2 TO Y-col  S" Vla"        SET-VLABEL
		   S" 50 Hz source frequency" SET-IXLINE
	    [THEN]

graph-id# 8 = [IF] -0.49913e -0.05e  4.49987e 0.05e DIMENSIONS
		   0 TO X-col  S" Time [s]"   SET-HLABEL
		   1 TO Y-col  S" Ila"        SET-VLABEL
		   S" 50 Hz source frequency" SET-IXLINE
	    [THEN]



